|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **INSTALLATION AND SAFETY INSTRUCTIONS**   |  | | --- | | **FINIAL ASSEMBLY** |   **STEP1:** After wires are connected, tuck them carefully inside outlet box.  **STEP2:** Put the back plate (E) on the mounting screw (C) and secure them with the ball finial (F).  **STEP3:** Put the glass shade (H) and spacer (I) on the socket (G), use socket wrench (M) to lock the socket ring (J) on them.  **STEP4:** Install the G9 bulb (K) on the socket (G) and lock the lamp shield (L) (**Do not use lamp shield (L) when using LED G9 bulbs**). See important Caution note below) on the socket (G).  **(CAUTION - USE TYPE G9 HALOGEN BULB WITH PROTECTIVE SHIELD. DISCONNECT POWER BEFORE SERVICING.)**   |  | | --- | | **CLEANING** |   To clean, wipe fixture with a soft cloth. Clean glass with a mild soap. Do not use abrasive materials such as scouring pads or powders, steel wool or abrasive paper**.**   |  | | --- | | **ORDERING PARTS** |   Keep this sheet for future reference, and in case you need to order replacement parts. All parts for this fixture can be ordered from place of purchase. Be sure to use exact wording from illustration when ordering parts.   |  | | --- | | **FOR YOUR SAFETY** |   **WARNING: BE SURE THE ELECTRICITY TO THE WIRES YOU ARE WORKING ON IS SHUT OFF; EITHER THE FUSE IS REMOVED OR THE CIRCUIT BREAKER IS SHUT OFF. GENERAL** You don’t need special tools to install this fixture. Be sure to follow the steps in the order given. Under no circumstances should a fixture be hung on house electrical wires, nor should a swag type fixture be installed on a ceiling which contains a radiant type heating system. Read instructions carefully. If you are unclear as to how to proceed, consult a qualified electrician. NOTE: Proper wiring is essential for the safe operation of this fixture.   |  | | --- | | **GENERAL** |   You don’t need special tools to install this fixture. Be sure to follow the steps in the order given. Under no circumstances should a fixture be hung on house electrical wires, nor should a swag type fixture be installed on a ceiling, which contains a radiant type heating system. Read instructions carefully. If you are unclear as to how to proceed, consult a qualified electrician.  **NOTE:** Proper wiring is essential for the safe operation of this fixture.   |  | | --- | | **FIXTURE ASSEMBLY** |   Carefully removed the fixture from the carton and check that all parts are included as shown in figure. Be careful not to misplace any of the screws or parts, which are needed to install this fixture.   |  | | --- | | **INSTALLATION** |   **IMPORTANT**: This fixture is only designed to mount with the bulbs and glass opening facing upwards, do not mount with the bulbs and glass openings facing downwards.  Do not attach fixture directly to outlet box.  **STEP1:** Thread the two fixture mounting screws (C) part way into  the universal mounting plate (B) and tighten with two hex nuts  (D). Install universal mounting plate (B) on the outlet box.  **STEP2**: Secure universal mounting plate (B) and outlet box with box screw(A).  Proceed to connect wires:  **GROUNDING INSTRUCTIONS**  **STEP 1**: Insert the green grounding screw into the hole with two raised dimples on the circular strap. Wrap the ground wire from the fixture (if supplied) around the green grounding screw, then connect it to ground wire from the outlet box (if not fixed on the outlet box) using a wire connector (not supplied). If ground wire from the fixture is not supplied, wrap the ground wire (if not fixed on the outlet box) from the outlet box around the green grounding screw and tighten it. **NEVER CONNECT GROUND WIRE TO BLACK OR WHITE POWER SUPPLY WIRES.**  **STEP 2:** Take note of the color of the wire(s) on your fixture.  Identify which group your fixture wire(s) falls into and connect the wires according to the directions below:  **NOTE:** When parallel wire (SPT-I & SPT-2) is used, the tracer wire is square shaped or ridged and the less tracer wire is round in shape or smooth (seen best when viewed from wire end.)  **STEP 3:** Take your fixture wire(s) from group A and place evenly against the black wire from the outlet box. Do NOT twist wires together before using wire connectors.  **STEP 4**: Fit a wire connector (not supplied) over the wires and screw the connector clockwise until you feel a firmness.  **STEP 5:** Try gently to pull the connector off the wires. If you can  pull the connector off, carefully re-do steps 3 and 4, as  above, and check again for a firm connection.  **STEP 6:** Connect the fixture wire from group B to the white wire  from the outlet box in the same manner. |

**Line art shown may not exactly match the fixture enclosed. However, the installations do apply to this fixture.**

**ITEM NO:1927-1S,1927-2V,1912-3V,1912-4V, 1912-5V**





|  |  |
| --- | --- |
| GROUP A: Connect to Black  House Wire | GROUP B: Connect to White  House Wire |
| BLACK | WHITE |
| \*PARALLEL WIRE (round & smooth)  smooth) | \*PARALLEL WIRE (square & ridged)  ridged) |
| WHITE OR GREY WITH TRACER | WHITE OR GREY WITHOUT TRACER |
| BROWN GOLD OR BLACK WITHOUT TRACER | BROWN, GOLD OR BLACK WITH TRACER |