|  |  |
| --- | --- |
|   **ASSEMBLY INSTRUCTIONS**

|  |
| --- |
| **LAMP ASSEMBLY** |

Carefully removed the lamp from the carton and check that all parts are included as shown in figure. 1. Connect the pipe (G) to the threaded nipple (F), pipe (D) should be on the top, attach the connected pipe to the threaded nipple on the lamp base (H).
2. Slide the lamp shade assembly (A) through top pipe (D).
3. Using the suction cup (E) to install the bulb (C) to lampholder (B).
4. Attach plug (L) to wall outlet.

Note: a) This floor lamp contains a touch sensor switch, it could be turn on/off by touching the part of lamp shade assembly (See Fig. 2), but the bottom parts are non-sensible.  b) Using the handle (K) to adjust the lamp shade angle, turning the knob (J) to adjust the height of lamp shade assembly.   |



Line art shown may not exactly match the fixture enclosed. However, the installations do apply to this fixture.

ITEM NO: 814-FL

`